BASKETBALL GOAL

	A.	Model No. 1000 Flex Goal as manufactured by Performance Sports Systems, Noblesville, IN.

	B.	Goal shall be fabricated from 5/8’’ diameter cold drawn alloy steel round formed to an 18’’ inside diameter ring. Inside of ring shall be positioned 6’’ from face of backboard by heavy, formed steel hinged-type housing with removable cover to conceal mounting bolts and shock absorption mechanism of goal and to protect against finger entrapment.

	C.	Goal shall defect in degrees according to applied pressure.	
 
	D.	Goal shall a continuous no tie ring with anti-whip net and hardware included. Universal goal mounting plate will fit the hole pattern for most 42” and 48” rectangular and most fan shaped backboards. 

	E.	Goal shall be finished in durable, electrostatic powder coated official orange finish. 

	F.	Goal shall be furnished complete with heavy-duty white anti-whip nylon netting and mounting hardware.