MANUAL WINCH

A.           Model No. 1123 Manual Winch by Performance Sports Systems, Noblesville, IN.

B.	       Manual winch shall be worm gear type designed to hold backstop at any position during        operation.  Winch shall be heavy-duty 1000 lb. capacity with ample, oversized flanges to prevent        cable from climbing drum ends.  40:1 worm gear ratio with long lasting ball bearing-type thrust        bearing and maintenance-free lifetime sealed gear case.  Input shaft shall not extend beyond        winch housing for safety.

C.          Manual winch drum shall be grooved for 1/4” 7 x 19 galvanized aircraft cable to facilitate smooth               take-up of and proper spooling of cable.  Drum shall be supplied with a pressure roller and               torsion spring tensioning to ensure cable tracks in grooves and to prevent bunching up and wear               and tear on cable, even in slack cable conditions. 

D.         Winch shall be provided with 2’’ x 10’’ x 30’’ yellow pine wood pad for mounting to wall. Pad              shall have chamfered edges and be finished with two coats of natural clear gloss lacquer.  Winch              shall be located so that backstop is in full view of authorized operator at all times.

	E.         Winch shall have two (2) year warranty against material defects and workmanship.  Any winch                          without this warranty does not meet these specifications and should not be considered. Winches                          with less than a two (2) year warranty or that require additional lubrication or maintenance shall                          not be considered equal.