MANUAL BASKETBALL BACKSTOP HEIGHT ADJUSTER

A. 	Model No. 1131 Manual Adjust-A-Goal by Performance Sports Systems, Noblesville, IN.

B.         Height adjuster shall be manufactured of steel using an Acme threaded screw rod with awning type hand crank to raise and lower backboard.  Height adjuster shall be screw driven to raise and lower goal height from 8’ to 10’ off of finished floor.  Screw drive shall be a 3/4’’ Acme double-start threaded rod secured in two bronze bushings.  Height adjuster shall be operated from floor by hand crank (included with height adjuster).   Adjust-A-Goal features a direct goal attachment to transfers load of play directly through backboard to support structure.