ELECTRIC BASKETBALL BACKSTOP HEIGHT ADJUSTER

A. 	Model No. 1171 Electric Adjust-A-Goal by Performance Sports System, Noblesville, IN.

B.	Electric height adjuster shall be manufactured of steel using an electrically operated linear actuator to raise and lower backboard from 8’ to 10’ off of finished floor.  Linear actuator shall be powered by a 115 volt single-phase motor and contain built in limit switches to ensure safe operation and positive stopping at 8' and 10' heights.  Adjust-A-Goal features a direct goal attachment to transfers load of play directly through backboard to support structure. Adjust-A-Goal shall be operated with a flush mounted single keyed switch (eliminating the need to two keys) or portable power wand.  Optional wireless remote control or keypad control operation available.