BASKETBALL GOAL

	A.	Model No. 2000+ Breakaway Goal as manufactured by Performance Sports Systems, Noblesville, IN.

	B.	Goal shall be fabricated from 5/8’’ diameter cold drawn alloy steel round formed to an 18’’ inside diameter ring. Inside of ring shall be positioned 6’’ from face of backboard by heavy, formed steel hinged-type housing with removable cover to conceal mounting bolts and shock absorption mechanism of goal and to protect against finger entrapment. 

	C.	Goal shall be designed to absorb shock loads from slam dunking or hanging on rim.  Shock absorption feature shall be provided by means of a special offset hinge arrangement rim and back plate mounting housing with concealed molded rubber shock absorber. 

	D.	Goal shall meet NCAA, FIBA and NFSHSA specification on moveable rims, which states, "A moveable basket ring shall have rebound characteristics identical to those of a non-moveable ring." Goal shall be factory set to proper flex and rebound requirements.

	E.	Goal shall be finished in durable, electrostatic powder coated official orange finish. 

	F.	Goal shall be furnished complete with heavy-duty white anti-whip nylon netting and mounting hardware.