BASKETBALL GOAL

	A.	Model No. 240 Double Ring Super Goal as manufactured by Performance Sports Systems, Noblesville, IN.

	B.	Goal shall be fabricated from 5/8’’ diameter top ring and ½” diameter bottom ring cold drawn alloy steel formed to an 18’’ inside diameter ring. Inside of ring shall be positioned 6’’ from face of backboard by heavy, formed steel. 

	C.	Goal shall be finished in durable, electrostatic powder coated official orange finish. 

	D.	Goal shall be furnished complete with heavy-duty white anti-whip nylon netting and mounting hardware.