BASKETBALL GOAL

	A.	Model No. 39WO Single Ring Stationary Goal as manufactured by Performance Sports Systems, Noblesville, IN.

	B.	Goal shall be constructed with an official size 18” ring of 5/8’’ diameter steel with twelve continuous no-tie net attachments. Back plate shall be 3/16” thick and 6 7/16” x 7”. Brace shall be 7/16” diameter all welded construction.  

	C.	Goal shall be finished in durable, electrostatic powder coated official orange finish. 

	D.	Goal shall be furnished complete with heavy-duty white anti-whip nylon netting and mounting hardware.