GYM DIVIDER CURTAIN
	
		A.	Model 4013 Walk Draw:  Manually operated, horizontal pull type gymnasium divider including clamps for attachment to building structure, and other components required for complete functional installation; Walk-Draw Gym Divider as manufactured by Performance Sports Systems, Noblesville , IN.

		B.	Operation:  Curtain suspended from overhead track and manually pulled open and closed while walking.

		C.	Configuration:  [Single] [2] [3] [4] [_____] curtain[s] arranged in [straight line] [curved] [box] [_____] shape as indicated on Drawings.  [Curtains to be bi-parting with [[3 feet] [914 mm] overlap at opening.] [velcro fasteners at opening.]] [Curtain to stack on one side.]  

			1.	Stack space for curtain shall not exceed 1-1/8 inches per carrier.

			2.	Minimum required clearance for curtain on each side of track: 6 inches.

		D.	Track:  16 gage galvanized steel channel-type track 1-1/2 by 1-1/4 inches attached to structural support [with beam clamps and hanger brackets] at 8 feet maximum on center.

		E.	Attachment:  Attachment:  Attach to structural support with beam clamps, hanger brackets, and 1/2 inch diameter threaded rods. Attachment clamps designed to be capable of supporting a minimum of 5,000 lbs each and provided in sufficient number to provide a combined minimum 45:1 attachment point safety factor.

		F.	Carriers: 1-1/8 inches diameter ball bearing wheels with trim chain for attachment to grommets in curtain top.  Space carriers at 12 inches.

		G.	Divider bottom:  Weighted with No. 2/0 coil proof chain in curtain pocket.