GYM DIVIDER CURTAIN
	
		A.	Model 4030 Roll-Up:  Electrically operated, roll-up gymnasium divider including motor, belts, controls, clamps for attachment to building structure, threaded rod supports, and other components required for complete functional installation; Roll-Up Gym Divider as manufactured by Performance Sports Systems, Noblesville, IN.

		B.	Operation:  Curtain rolled up and down by belts wound onto overhead rotating drive pipe operated by electrical motor.

		C.	Configuration:  Rectangular shape with straight bottom and extending across room as indicated on Drawings.

			1.	Maximum dimension of stored divider: 2 feet from bottom of structural support to bottom of rolled curtain.

			2.	Minimum required clearance between vertical curtain edges and adjacent fixed objects: 6 inches.

			3.	Provide 36 inches space between curtain ends and walls or fixed objects to allow passage space around divider.

		D.	Operating mechanism:  Drive pipe winch powered with 1 HP, 110VAC, 60-cycle, single-phase, reversible capacitor, C-Face motor with thermal overload protection.  Entire winch assembly to be UL listed and shall carry a five-year warranty.  Provide with load holding worm gear reduction and integral limit switches to control curtain travel.  Drive pipe shall rotate in pipe support assemblies spaced at approximately [9 feet] [2.7 m].

		E.	Attachment:  Attach to structural support with beam clamps, hanger brackets, and 1/2 inch diameter threaded rods. Attachment clamps designed to be capable of supporting a minimum of 5,000 lbs each and provided in sufficient number to provide a combined minimum 45:1 attachment point safety factor. 

		F.	Hoist belts: 4 inches wide black polyester webbing attached to drive pipe, passing under bottom batten, and terminating at top batten.  Space belts at approximately 15 feet. 

		G.	Bottom roller: 3-1/2 inches diameter steel pipe with aluminum strip for attachment of curtain.