3.6	PROTECTIVE WALL PADDING

	A.	Model No. 4120 by Performance Sports Systems, Noblesville, IN.

	B.	Panels are 2’ wide by 6’ high, with custom sizes available.  Panels shall be constructed of 2’’ thick 6 lb. density bonded foam. Each panel shall be covered with 14 oz. polyester reinforced laminated vinyl and cemented to 7/16’’ OSB exterior grade wood panels with one-inch nailing margins at top and bottom (for securing panels to wall). Available in fifteen (15) standard colors (color to be determined by Architect).  All cutouts in panels shall be made in field to fit job conditions. 

	C.	Vinyl flammability rated as self-extinguishing by the California State Fire Code. 

		Available Options:
		Custom Heights and Widths
		1 ½” Foam
		½” Fire Rated Plywood Backer
		Vonar,