3.6	PROTECTIVE WALL PADDING

	A.	Model No. 4130 Class “A” Fire Rated Neoprene Foam Wall Padding by Performance Sports Systems, Noblesville, IN.

	B.	Panels are 2’ wide by 6’ high, with custom sizes available.  Panels of 2’’ thick CR Safguard fire retardant neoprene foam meeting ASTM E84 with Class A rating flame spread index of 25 or less, and smoke development index of 450 or less. Each panel shall be covered with 14 oz. polyester reinforced laminated vinyl and cemented to 7/16’’ OSB exterior grade wood panels with one-inch nailing margins at top and bottom (for securing panels to wall).  Available in fifteen (15) standard colors (color to be determined by Architect).  All cutouts in panels shall be made in field to fit job conditions. 

	C.	Vinyl flammability rated as self-extinguishing by the California State Fire Code.
		
		Available Options:
		Custom Heights and Widths