RECTANGULAR GLASS BACKBOARDS

	A.	Model No. AFRG42E Aluminum Framed Rectangular Glass Backboard by Performance Sports Systems, Noblesville, IN. 

	B.	Backboards shall be 42 inches high by 72 inches wide.

	C.	Backboard shall be manufactured from 1/2” tempered glass set in heavy extruded aluminum  framing and cushioned by shock absorbing vinyl.  Official border and target area permanently fired into glass.  

	D.	Goal mounting structure shall be a heavy welded formed steel assembly, and directly attached to lower horizontal frame member to minimize stress on glass. 

E.	       Backboard shall have 10 year warranty against defects in material and workmanship, and        when used with Performance Sports System’s Direct Goal Attachment feature shall be protected        against shatter and breakage of glass. Board must meet NCAA, FIBA and NFSHSA        specifications.