GROUP CONTROLLER – Model TSC1500XL-WiFi Wireless Controller by Performance Sports Systems, Noblesville IN. 

The TSC1500XL WiFi Control system shall be an alternate to conventional key switch type controls. The system shall be designed to operate backstops, divider curtains, electric height adjusters, overhead volleyball systems, batting cages and power control for auxiliary gymnasium electrical equipment such as lighting, scoreboards, etc. The system shall include a 5.7” color touch screen that is wirelessly controlled by any smart phone or a tablet device connected to the system generated network with a proprietary software application (any system that operates off a network other than one generated by the system itself will not be considered equal). The system shall be password controlled to prevent unauthorized use. The system shall allow for an infinite number of user logins to be created all with their own alpha numeric passwords. The system shall be designed with a one touch “Press and hold” button operation to prevent authorized operators from walking away while equipment is in motion. System shall allow control of auxiliary equipment with a single press of the pad. Control pad shall auto shut-off after thirty seconds of non-use.  
		The system shall include one 18” wide x 24” tall x 6” deep relay box with twenty four relays per box capable of operating up to twelve devices total. System shall be capable of operating all twelve devices simultaneously when adequate power is provided. Systems that cannot operate twelve devices simultaneously will not be considered equal. The system shall be expandable up to 16 relay boxes until 192 devices are reached. 

The system shall operate on 110 Volts with screen communications at 24 Volts DC.  System will operate equipment individually and has user interface for multiple equipment configurations and operation. Systems that do not allow for multiple equipment configurations and operation will not be considered equal

	Manual Control override with 15’ cord, which is to be used at the relay panel as a back-up to the touch screen (Any control system that does not include a manual control override will not be considered equal). 

	All other electrical, junction and synchronizer boxes not mentioned above to be furnished and installed by a certified electrical contractor.  Follow manufacturer’s instructions and all local safety codes

Wiring of all electrical components shall be in accordance with local codes, and in accordance with manufacturer’s instructions.  All conduit, wiring, junction boxes, and components not specified shall be furnished and installed by electrical contractor.  In addition, relay panel dip switch settings and relay set programming per the facilities requirements shall be the responsibility of the electrical contractor.