PADDED REFEREE STAND

A.	Model 6446 Referee Stand - 1” square tubular steel construction, stand shall have self be self-supporting on four legs with safety bars 34” above the platform. The referee stand shall have the ability to be converted, by removing front legs, to a tri-pod design supported by means of a V-bracket and velcro strapped to the volleyball post as manufactured by Gared Sports, Noblesville, IN.

	Model 6040 Referee Stand Padding – Padding designed to cover the legs, braces, and platform edge. Padding shall be a min.1” thick cross-linked polyethylene closed cell foam covered with 14-oz. nylon reinforced vinyl. Colors available are white, yellow, orange, red, kelly green, forest green, royal blue, marine blue, navy blue, gray, black, maroon, beige, teal, and purple.