BASKETBALL EQUIPMENT

	Model 9305 Gared Hoopmaster LT Portable Basketball Backstop as manufactured by Gared Sports, 
	Noblesville, Indiana.
	
	A.	Frame: The base of the frame shall be constructed of tubular steel members 2”x3”x 1/8” to form a single heavy duty unitized frame. The vertical mast and horizontal extension “boom” shall be formed from 3” square steel sections diagonally braced by 2” structural steel tubing sections for maximum rigidity. Upper and lower ends of vertical supports shall pivot in adjustable, oil impregnated bronze type bushings for maintenance free operation. All pipe and tubing shall meet or exceed ASTM A513 structural steel specifications. The boom shall length shall extend 8’ from the front of the unit to the face of backboard. The front of the frame shall be fitted with a positioning pin at both sides to guarantee correct placement during play. Unit shall lock on the floor by means of four (4) foot operated, retractable, positioning floor locks.

		Height Adjustable between 10’ to 8’

	B.	Ballast: Each unit shall have a minimum ballast weight of 950lbs. permanently built into the rear of the unit. 

			C.	Wheels: Base shall be equipped with four (4) heavy duty, non marking, 5” diameter ball bearing swivel castors with  grease fittings for internal lubrication.

D.	Anchors: Each unit shall be furnished with a floor anchoring system to lock the unit down in the 
back of the backstop per NCAA specifications.	

E.	Padding: Main vertical mast, horizontal boom extension and front area shall be padded with a 2” 
thick heavy duty polyurethane foam and covered with a 14oz. tear resistant vinyl. All padding shall be attached in a manner allowing quick replacement.

	F.	Finish: All exposed metal surfaces will be White Baked On Powder Coat finish. Custom Colors are available as an add option.

G	Folding Cycle: Each unit shall be raised by four heavy duty tension springs located in the base. An additional fifth spring will be required if the unit includes a shot clock mount. The maximum effort to raise or lower the unit shall be sixty pounds applied by one person at the handle provided on the rear upright. A telescoping locking bar with a safety locking pin shall be used to hold the unit in full up and full down position.
	
H.	Goal and Backboard Attachment: The goal and backboard shall utilize a direct goal attachment completely eliminating the stress on the glass. 

	RECTANGULAR GLASS BACKBOARDS

	A.	Model No. BB72G50 Aluminum Framed Rectangular Glass Backboard Gared Sports Systems Inc., Noblesville, IN. 

	B.	Backboards shall be 42 inches high by 72 inches wide.

	C.	Backboard shall be manufactured from 1/2” tempered glass set in heavy extruded aluminum or steel framing and cushioned by shock absorbing vinyl.  Official border and target area permanently fired into glass.  

	D.	Goal mounting structure shall be a heavy welded formed steel assembly, and directly attached to lower horizontal frame member to minimize stress on glass. 

E.	       Backboard shall have limited lifetime warranty against defects in material and workmanship, and        when used with Performance Sports System’s Direct Goal Attachment feature shall be protected        against shatter and breakage of glass. Board must meet NCAA, FIBA and NFSHSA        specifications.

F.	       Provide Model No. 1330 Pro Mold Bolt-On Cushion Edge by Performance Sports Systems        Inc., Noblesville, IN. Available in ten (10) standard colors (color to be determined by Architect).         Five (5) year warranty.

2.5	BASKETBALL GOAL

	A.	Model No. 2000+ Breakaway Goal as manufactured by Performance Sports Systems Inc., Noblesville, IN.

	B.	Goal shall be fabricated from 5/8’’ diameter cold drawn alloy steel round formed to an 18’’ inside diameter ring. Inside of ring shall be positioned 6’’ from face of backboard by heavy, formed steel hinged-type housing with removable cover to conceal mounting bolts and shock absorption mechanism of goal and to protect against finger entrapment. 

	C.	Goal shall be designed to absorb shock loads from slam dunking or hanging on rim.  Shock absorption feature shall be provided by means of a special offset hinge arrangement rim and back plate mounting housing with concealed molded rubber shock absorber. 

	D.	Goal shall meet NCAA, FIBA and NFSHSA specification on moveable rims, which states, "A moveable basket ring shall have rebound characteristics identical to those of a non-moveable ring." Goal shall be factory set to proper flex and rebound requirements.

	E.	Goal shall be finished in durable, electrostatic powder coated official orange finish. 

	F.	Goal shall be furnished complete with heavy-duty white anti-whip nylon netting and mounting