WALL MOUNTED UP FOLDING BACKSTOPS

A.	Model No. 2400 (4’min. – 12’ max. extensions) Wall Mounted Up Folding Basketball Backstop as manufactured by Performance Sports Systems, Noblesville, Indiana.

	B.	“Wall Mount Structure” four 1 7/8” O.D. tubes telescoped inside 2 1/8” O.D. tubes, spaced at 63” centers for standard application and 35” centers for fan shaped backboards. Unit shall be cross braced with ¼”x1” tension strap fastened to structure. All critical fittings shall be malleable iron castings, heavy gauge steel stampings, or weldments. Backstop manufactured in accordance with all NCAA, NFHS, NBA requirements. 

 	C.	Unit shall attach to 2”x7.25” clear coated wood pads. Unit will be supported with 4/0 chain fastened to front of the unit and attached to a wood pad mounted on the wall. Wood pad will be mounted on an 8” min. solid core concrete block wall or will of similar integrity. All critical fittings shall be malleable iron castings, heavy gauge steel stampings, or weldments.

	D.	All metal parts shall have factory applied powder coat finish in standard black. Available colors: white, blue, red, gray, and yellow. 

	E.	Unit shall be operated with a Model 1123 Manual Winch.