3.5		Badminton 
		Model 6619 Single Court Badminton Game system consists of one pair of 2-3/8" O.D. sleeve type posts with sliding net tensioning collars. Posts are 3/16" wall high strength mechanical tubing furnished with all necessary hardware. Post and sliding tensioning net collars are powder coated black. The net (502102) is made of rugged #12 nylon, brown flexabar treated for extra durability. It has white top binding with nylon taped sides and bottom with twisted poly rope in top binding
feature a 1' diameter wood dowel.  The net must meet NCAA, NFSHSA and USVBA specifications

3.5	NET ANTENNA

	A.	Model No. 6412 antenna by Gared Sports, Noblesville, IN.

	B.	Antennae is secured firmly to the net by insertion in the full length pockets in then sidelines markers fully eliminating the possibility of the antennae dislodging from the net.