FUTSAL GOAL

A.	Model 8300 Single net storage system as manufactured by Gared Sports, Noblesville IN. Upright posts and cross bar are constructed of 8 cm square extruded aluminum tubing. Backstays and rear stabilizing bar constructed of 1 5/8” O.D.  heavy wall galvanized tubing. Standard finish is white powder coat on main goal frame. (Optional finish is natural, unpainted).

	Official size goal measures 3m between uprights, 2m between crossbar and floor, and 1m deep.

	Meets FIFA and U.S. Futsal specifications.

	Goal includes sand bags for ground weighted rear stabilizer bar and net.