GROUP CONTROLLER

		Model No. TSC1500XL Group Controller as manufactured by Performance Sports Systems, Noblesville, IN.
		
A.	Wall mounted touch screen control system shall be designed as an alternate to conventional key switch type controls, to operate backstops, divider curtains, electric height adjusters, overhead volleyball systems, batting cages, and power control for auxiliary gymnasium electrical equipment such as lighting, scoreboards, etc.  Control system can operate a maximum amount of 192 devices and a maximum of 50 auxiliary devices.
B.	The TS1500XL uses a 5.7” touch screen in an 8” wide x 8” tall x 4” deep enclosure. The screen will display the requested gym layout with easy to understand controls for proper selection of items to operate.
C.	Gym equipment can be operated individually or in multiple equipment configurations with the ability to operate as many devices at one time as the end user require as long as each device is on it’s own dedicated 20amp circuit.